## General Settings

Location:

The location is required to determine the time zone, daylight saving, sun rise/set and the weather. If it is not set AEST time will be used.

City Name: Country Code:
{ LocationTestMsg} { LocationDataMsg}
The country code is generally the first two letters of the country (called the ALPHA-2 code), click here for the full list. Use the TEST button to test the settings. If you cannot find your city try a nearby larger city and if that fails chose a city in the same timezone with the same daylight saving rules.

Sensors:

Detect Abnormal Water Flow: | Enable | {ResetFlowMsg}
Installed Rain Sensor: | Enabled | (contacts open on rain)

Detecting abnormal water flow requires that a flow meter be installed at the pump or master valve outlet with its output signal connected to the flow input terminal.

Logging:

Status information can be logged to the file log.txt:
"Log Significant Events" will log just watering events and errors.

Email Settings:

Emails are optional. To send emails an account must be opened with an SMTP relay service. You can use either SMTP2GO or SendGrid (not both). Leave the one that you are not using blank.

SMTP2GO: Create a free account at https://www.smtp2go.com/, register a Verified Sender and create an associated username and password and enter them below: Username: Password:

SendGrid: Create a free account at https://sendgrid.com, then create an API key (a 69 character string starting with SG) and paste it into the field below.
API Key:

Enter the sender address and the recipient (they can be the same). Note that the sender (ie, the From Address) must be the same as that registered with the SMTP relay service.

From Email Address:

To Email Address:

Notifications:
Send email if unable to get the current time/date
Send email if unable to get the weather forecast
Send email if abnormal water flow is detected

{EmailTestMsg}

{ SavedMsg}